Configuration	car
STM32CubeMX 	4.16.1
Date	01/18/2018
MCU	STM32F103C8Tx



PERIPHERALS	MODES	FUNCTIONS	PINS
CAN	Master	CAN_RX	PA11
CAN	Master	CAN_TX	PA12
RCC	Crystal/Ceramic Resonator	RCC_OSC_IN	PD0-OSC_IN
RCC	Crystal/Ceramic Resonator	RCC_OSC_OUT	PD1-OSC_OUT
SYS	Serial Wire	SYS_JTCK-SWCLK	PA14
SYS	Serial Wire	SYS_JTMS-SWDIO	PA13
SYS	SysTick	SYS_VS_Systick	VP_SYS_VS_Systick
TIM2	ETR2	TIM2_ETR	PA0-WKUP
TIM3	Internal Clock	TIM3_VS_ClockSourceINT	VP_TIM3_VS_ClockSourceINT
TIM3	PWM Generation CH1	TIM3_CH1	PB4



Pin Nb	PINs	FUNCTIONs	LABELs
2	PC13-TAMPER-RTC	GPIO_Output	LED
3	PC14-OSC32_IN	GPIO_Output	ERROR
4	PC15-OSC32_OUT	GPIO_Output	LED2
5	PD0-OSC_IN	RCC_OSC_IN	
6	PD1-OSC_OUT	RCC_OSC_OUT	
10	PA0-WKUP	TIM2_ETR	Tacho_In
32	PA11	CAN_RX	
33	PA12	CAN_TX	
34	PA13	SYS_JTMS-SWDIO	
37	PA14	SYS_JTCK-SWCLK	
40	PB4	TIM3_CH1	PWM_Out
41	PB5	GPIO_Output	HighSideEn
42	PB6	GPIO_Output	LowSideEn



SOFTWARE PROJECT

Project Settings : 
Project Name : car
Project Folder : /home/wn/workspace-stm32/car/cubemx/car
Toolchain / IDE : SW4STM32
Firmware Package Name and Version : STM32Cube FW_F1 V1.4.0


Code Generation Settings : 
STM32Cube Firmware Library Package : Copy only the necessary library files
Generate peripheral initialization as a pair of '.c/.h' files per peripherals : No
Backup previously generated files when re-generating : No
Delete previously generated files when not re-generated : Yes
Set all free pins as analog (to optimize the power consumption) : No


Toolchains Settings : 
Compiler Optimizations : Balanced Size/Speed






